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15th RHN REGATTA 2026

October 31 - November 7 , Sanya, Hainan, China

Category 3 + Liferaft: Races across open water, most of which is relatively protected or close to shorelines. (OSR 2.01.4)
The present inspection card is based on World Sailing Offshore Special Regulations (OSR) 2026-2027 and do not cover ALL
rules of OSR. The full compliance with OSR Category 3(www.sailing.org) is the sole responsibility of the person in charge
and it cannot be limited to the present inspection card (OSR 1.02). The OSR do not replace, but rather supplement, the
requirements of governmental authority, or any other rules or regulations (OSR 1.01.2).

Safety Checklist

BOAT [ ]

OOO0O00O0O
.

MMSI Number

CREW Number

C] SPARE NAVIGATION LIGHTS

D MARINE TRANSCEIVER or VHF + emergency antenna

when the regular antenna depends upon the mast

D HAND-HELD MARINE VHF

D FLASHLIGHT & SEARCHLIGHT

Minimum IP67 rated of at least 400 Lumnens

D FIRST AID MANUAL & FIRST AID KIT

D PYROTECHNIC SIGNALS

2 orange smokes + 4 red hand flares

D BILGE PUMP + handle / 2 BUCKETS with lanyard

MEASURER , ]

DATE ( ]

D 2 ANCHORS with suitable combination of CHAIN and ROPE

D TETHERS not exceeding 1m or if 2m meters need to have an

intermediate self-closing hook + overload indicator

D LIFEJACKETS (with crotch / thigh strap / spray hood / light)

+ spare gas bottle or spare lifejacket

D GRAB BAG

D PULPITS, STANCHIONS and LIFELINES

All lifelines in stainless steel wire, Dyneema is NOT allowed
D JACKSTAYS and CLIPPING POINTS
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ORC

STABILITY

OSRreference 304 /3.04.2b)
Stability in accordance to OSR 3.04
(e.g. ORC Stability Index > 103).

VHF with MASTHEAD ANTENNA
and spare antenna

OSRreference 3295

Marine radio transceiver with an
emergency antenna when the regular
antennadepends upon the mast. If VHF
min power of 25W, andf it's installed
after 31/12/2015,be DSC capable with
anassigned MMSI (unique to the boat)
&connected to GPSreceiver.

SOFT TAPERED WOOD PLUGS
OSRreference 4.03

Soft tapered wood plugs attached
oradjacent to the appropriate fitting
for every through-hull opening.

ORC

BALLAST OR GENERATOR
OSRreference204.2/3.28.2

If ballast or generator exists: must be per-
manently installed. Heavy items securely
fastened.

HAND-HELD MARINE VHF with
VHF stored in the Grab Bag
OSRreference 3.291

Hand-held marine VHF transceiver,
watertight or with a waterproof

cover. When notin use to be stowedina

grab bag.

FIRE EXTINGUISHERS (2X 2Kg)
FIRE BLANKET

OSRreference 4.051/4.05.2

2fire extinguishers, = 2kg, dry powder,
accessible, different positions. Fire blan-
ket near cooking device of open flame.

NAVIGATIONLIGHTS
OSRreference 3.27

Navigation lights mounted above
sheerline +reserve lights that can be
powered independently, spare bulbs
(not required for LED).

SeanglEne

AIS TRANSPONDER & GPS
OSRreference 3.29.7/3.29.8/

AIS Transponder sharing VHF
masthead antenna or with a dedicated
AlS antennaanda GPS.

AIS shallbe active from the first day of
equipment inspection until the end of
theevent.

FLASHLIGHTS and SEARCH-
LIGHTS

OSRreference 407

Watertight lights (minimum IP67 rated)
with spare batteries and bulbs as
follows, or awatertight (minimum IP67
rated) rechargeable LED torch, of at
least 400 Lumens. Stowedineachgrab
bag.




image3.png
2026 - 2027 Offshore Special Regulations Category 3 + Liferaft

FIRST AID MANUAL and FIRST
AIDKIT

OSRreference 4.08

AFirst Aid Manual and First Aid Kit. The
contents and storage of the First Aid Kit
shall reflect the likely conditions and du-
ration of the passage, and the number
of crewmembers.

CHARTS & COMPASS
OSRreference4111/3.24

Navigational charts (not solely electronic),
and chart plotting equipment.
Permanently installed marine magnetic
steering compass, independent of any
power supply, correctly adjusted with
deviation card.

BUCKETS

OSRreference 3.231a)

Two strong buckets, each with alanyard
andofatleast 91(2.4 US Gal) capacity.

FOGHORN / RIGGING CUTTER/
STRONG KNIFE

OSRreference 409/416.2/4.25
Foghorn. Rigging cutter. Knife strong,

securely restrained, readily accessible from

the cockpit.

PYROTECHNIC SIGNALS
OSRreference 4.23
Pyrotechnic signals:

4 red handflares, 2 orange smokes.

\

ANCHORS
OSRreference 4.061

Two unmodified anchors with suitable

combination of chain and rope,
ready forimmediate assembly,and

ready for deployement within 5 minutes,
except for boat less than 8.5m LH there

shallbe 1anchor meeting the same
criteria.

RADAR REFLECTOR
OSRreference 410

Radar reflector: octahedral (with plates
circular 12" or rectangular 16”) or of
min2m2 radar cross-section.

e

BILGE PUMP

OSRreference 3231¢)

Bilge pump, manual, permanently
installed, operable with all cockpit
seats. Removable bilge pumps handle
retained by lanyard.

SAFETY HARNESS AND TETHERS
OSRreference 5021/502.2/502.3/
5025

Anharness shall complies with1SO 12401 or
equivalent. A tether shall complies withISO
12401 or equivalent. A tether shallhave overload
indicator flagembedded in the stitching andbe
manufactured after 2000.

All of the crew shall have either:a tether not
exceeding Im(33") including the length of the
hooks, or anintermediate self-closinghook on
a2m (6-6") tether. A tether whichhas been
overloaded shallbereplaced.
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LIFEJACKETS

OSRreference 501/501.2/5014

If manufactured before 2012 shall comply with ISO 12402 - 3 (Leve! 150) or equivalent, including EN 396 or UL 1180, if inflatable have
agasinflation system, hand be fitted with a whistle, lifting loop, reflective material automatic/manual gas inflation system, crotch/thigh
straps (ride up prevention system (RUPS)) If manufactured after 2011 shall comply with ISO 12402-3 (Level 150) and be fitted with a
whistle, lifting loop, reflective material automatic/manual gas inflation system, crotch/thigh straps (ride up prevention system (RUPS)).

All Lifejackets shall have an emergency position indicating lightinaccordance with either ISO 12402-8 or SOLASLSA code 2.2.3,

be clearly marked with the boat's or wearer's name, have a spray hood inaccordance with ISO 12402-8.

Aboat shall carry atleast one gas inflatable lifejacket spare cylinder.
i
GRABBAG

E i?
OSRreferences 4211/ 4214

Agrab bag for each liferaft shall have inherent flotation, at least 01 m? (1ft2) area of highly visible colour (e.g. dayglo yellow or orange) on the
outside, shall be marked with the name of the boat, and shall have a lanyard and clip, with the following minimum contents:

watertight hand-held marine VHF transceiver (same one from 3.291)

watertight flashlight with spare batteries and bulb (same one from 4.07)

3hand flares in addition to Pyrotechnic signals required by 4.231

awatertight strobe light with spare batteries (may be part of the flashlight) (same one from 4.07)

knife / whistle.

LIFEBUOY HEAVING LINE RECOVERY SLING
OSRreference4.22.3a) OSRreference 4224 OSRreferences 4.225

Lifebuoy near the helmsman with AHeaving line 15-25mlong, diameter > Recovery sling marked with the boat's
self-igniting light, yacht's name, retro-re- 6mm, readily accessible to cockpit. or wearer's name g with (a) buoyant
flective material and adrogue. line of length no less than the shorter of

4xLOAor 36m, (b) buoyancy section
(horseshoe) with > 90N buoyancy and
(c) minimum strength capable to hoista
crew member aboard
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PULPITS, STANCHIONS and LIFELINES

OSRreference 314

Lifelines: Two (for LOA = 8.5m) or One (for LOA < 8.5m), uncoated stainless steel wire.
Alanyard of synthetic rope may be used with gap not exceeding 100 mm. When ade-
flecting force of 4kgis applied to a lifeline at the mid-point of the longest span between
supports that are aft of the mast, the deflection shall not exceed: 50 mm (2") for an upper or
single lifeline 120 mm (434”) for an intermediate lifeline.

Lifelines permanently supported at intervals of not more than 2.2 m (7-21/2") and not
passing outboard of supporting stanchions.

HEAVY WEATHER JIB
OSRreference4.26.2/4.271/ 4273

With an area, in unreefed condition, of
13.5% height of the foretriangle squared,
and b) readily available method, independ-
entof aluff groove, to attach to the stay.

STORM TRYSAIL or REEFABLE
MAINSAIL

OSRreference 4.261/4.271/ 4.27.2
Either astorm trysail or Mainsail reefing to
reduce the luff by at least 40%

The storm trysail area calculated as:

(05 xleech length x shortest distance
between tack point andleech).

JACKSTAYS / CLIPPING POINTS
OSRreference 404

Jackstays shallbe independent on each
side of the deck. Clipping points adjacent to
the elm, sheets whinches and mast.

ORC

EMERGENCY TILLER &
EMERGENCY STEERING
OSRreference 415/ 4152

Emergency tiller capable of being fitted to
the rudder stock except when the principal
method of steering is by means of anun-
breakable metal tiller or there are two meth-
ods (tillers, wheels) of controlling a rudder,
neither of which shares components with
the other except for the rudder stock.

INFLATABLE LIFERAFTS -1S0 9650 Liferafts can not be stowed below deck!

RIGID CONTAINER LIFERAFT STOWAGE OSRreference 4.20/4.201/4.20.3
One or more inflatable liferafts ISO 9650
with a total capacity to accommodate
- arigid container securely stowed onthe atleast the total number of people on board.
working deck, inthe

cockpit orinan openspace

SOFT TYPELIFERAFT STOWAGE

-if avalise type (soft type bag) securely
stowedin adedicated weather tight locker
in the cockpit containing Liferaft and aban-
donship equipment only which is readily
accessible and opens onto the cockpit or
working deck, or transom.




